**Egocentric Camera – Basic User guide**

|  |  |
| --- | --- |
| **[INSERT CONTACT INFORMATION OF THE RESEARCH TEAM]** |  |

|  |
| --- |
| **POWER ON / OFF** |
| Press the Mode button for two seconds [ ] |  |
| **START / STOP RECORDING** |
| **Using the camera touch display:**Tap the icon in the lower left corner of the touch display |  |
| **Using camera remote:**1. Pair camera Remote to camera (For most cases, this should already be paired out of the box):
* From the main screen, swipe down from the top to bring up the menu and then select connect.
* From the connect menu select “Connect New Device”
* Now select the option “(Voice Remote)” A new message will appear on the camera screen asking you to power on the Remote. Set the camera aside.
1. Power on the remote by pressing hold the small power button on the side of the remote for 8 seconds.
2. From the main screen, swipe down from the top to bring up the menu and then select connect.
 | Image result for how to use gopro remote hero 5 |
| **Using camera Apps:**Live preview, playback and full camera control (including start and stop recording) can be operated from the camera Apps. | Image result for start stop recording gopro using app |
| **CHARGING THE BATTERY** |
| 1. Hold down the Latch Release button on the side door (if available), then slide the door open.
2. Connect the camera to a computer or other USB charging adapter using the included USB-C cable.
3. Power off the camera. The camera status light turns on during charging and turns off when charging is complete. When charging with a computer, be sure that the computer is connected to a power source. If the camera status light does not turn on, use a different USB port.
 |  |
| **VIEWING VIDEOS** |  |
| **Using the camera touch display:**1. Swipe right to open the gallery. If your microSD card contains a lot of content, it might take a minute for it to load.
2. Scroll through the thumbnails. Note: For photo series (Burst, Time Lapse, Night Lapse and Continuous photos), the thumbnail displays the first photo in the series.
3. Tap a video or photo to open it in full-screen view.
4. To add a HiLight Tag, tap []. HiLight Tags make it easy to bookmarks videos for later retrieval.
5. To return to the thumbnails screen, tap [].
6. To exit the gallery, swipe down.
 | GoPro Hero5 Tips |
| **Using camera Apps:**Live preview, playback and full camera control can be operated from the camera Apps. | Image result for start stop recording gopro using app |
| **DELETE SELECTED VIDEO FILES** |
| **Using microSD card:**1. connect the card reader to the computer
2. Remove microSD card from the camera:
* Hold down the Latch Release button on the battery door, then slide the door open.
* To remove the card, press it into the slot with your fingernail and it will pop out.
1. Insert the microSD card into the microSD slot/reader on your computer or the tablet provided (via File Manager App):
* The microSD card slot (accepts up to 128GB capacity cards) on the tablet, can be found under the rear cover.

 Image result for File Manager app asus File Manager 1. Delete selected video files on your card
 | Image result for asus 8 microSD card slotThe microSD card slot (accepts up to 128GB capacity cards), and SIM card slot can be found under the rear cover. The contacts below the slots is for the optional Audio Cover (more about this later). |
| **Using USB cable:**1. Connect the camera to your computer using the included USB-C cable
2. Power on the camera and follow the on-screen instructions
3. Delete selected video files on your card
 | Image result for connect gopro hero 5 to pc |